**Hybrid spot data sheet**

Hybrid profile offer a highly flexible 230v system for an almost tool-free installation. With a width range of Lumineers and accessories, this system offers a numerous applications option, combinations and solutions, even also for a corridor function.

The Hybrid spot is based on aluminium and thermoplastic. The aluminium gives the spotlight a very good passive dissipation, which provide a very long lifespan. Integrated in the thermoplastic adapter, there is Wieland connectors for easy connection and a Dali driver, which offer a full control and dimmable function. The swivel joints allow the spot to rotate 355° and tilt **??°.** With high efficiency reflectors, which is position deep in the spot, the Hybrid spot provide a high level of visual comfort and low glare.

**Hybrid linear data sheet**

Hybrid profile offer a highly flexible 230v system for an almost tool-free installation. With a width range of Lumineers and accessories, this system offers a numerous applications option, combinations and solutions, even also for a corridor function.

The Hybrid linear is based on aluminium and thermoplastic. The aluminium gives the luminaires a very good passive dissipation, which provide a very long lifespan. Integrated in the thermoplastic adapter, there is Wieland connectors for easy connection and a Dali driver, which offer a full control and dimmable function. With high efficiency prismatic cover, the Hybrid linear provide a high level of visual comfort and low glare.

**Hybrid dark light data sheet**

Hybrid profile offer a highly flexible 230v system for an almost tool-free installation. With a width range of Lumineers and accessories, this system offers a numerous applications option, combinations and solutions, even also for a corridor function.

The Hybrid dark light is based on aluminium and thermoplastic. The aluminium gives the luminaire a very good passive dissipation, which provide a very long lifespan. Integrated in the thermoplastic adapter, there is Wieland connectors for easy connection and a Dali driver, which offer a full control and dimmable function. With high efficiency reflectors, which is position deep in the luminaire, the Hybrid dark light provide a high level of visual comfort and low glare.

**Hybrid pendant data sheet**

Hybrid profile offer a highly flexible 230v system for an almost tool-free installation. With a width range of Lumineers and accessories, this system offers a numerous applications option, combinations and solutions, even also for a corridor function.

The Hybrid pendant is based on aluminium and thermoplastic. The aluminium gives the luminaire a very good passive dissipation, which provide a very long lifespan. Integrated in the thermoplastic adapter, there is Wieland connectors for easy connection and a Dali driver, which offer a full control and dimmable function. With high efficiency reflectors, which is position deep in the luminaire, the Hybrid pendant provide a high level of visual comfort and low glare.